'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_io.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_io.d" -MT"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_io.o" -o "Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_io.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_io.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_io.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_lcd.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_io.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_io.d" -MT"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_io.o" -o "Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_io.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_io.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_io.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_lcd.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_lcd.d" -MT"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_lcd.o" -o "Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_lcd.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_lcd.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_lcd.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_sdram.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_sdram.d" -MT"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_sdram.o" -o "Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_sdram.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_sdram.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_sdram.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_ts.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_ts.d" -MT"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_ts.o" -o "Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_ts.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_ts.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_ts.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/Components/ili9341/ili9341.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Drivers/BSP/Components/ili9341.d" -MT"Drivers/BSP/Components/ili9341.o" -o "Drivers/BSP/Components/ili9341.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/Components/ili9341/ili9341.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/Components/ili9341/ili9341.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/Components/stmpe811/stmpe811.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Drivers/BSP/Components/stmpe811.d" -MT"Drivers/BSP/Components/stmpe811.o" -o "Drivers/BSP/Components/stmpe811.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/Components/stmpe811/stmpe811.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/Components/stmpe811/stmpe811.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Application/User/BASIC_HelloWorld.d" -MT"Application/User/BASIC_HelloWorld.o" -o "Application/User/BASIC_HelloWorld.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c"
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:108:12: warning: 'v_stand_by_time_u8' initialized and declared 'extern'
  extern u8 v_stand_by_time_u8      = BME280_INIT_VALUE;
            ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:110:13: warning: 'v_data_uncomp_temp_s32' initialized and declared 'extern'
  extern s32 v_data_uncomp_temp_s32 = BME280_INIT_VALUE;
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:112:13: warning: 'v_data_uncomp_pres_s32' initialized and declared 'extern'
  extern s32 v_data_uncomp_pres_s32 = BME280_INIT_VALUE;
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:114:13: warning: 'v_data_uncomp_hum_s32' initialized and declared 'extern'
  extern s32 v_data_uncomp_hum_s32  = BME280_INIT_VALUE;
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:116:13: warning: 'v_comp_temp_s32' initialized and declared 'extern'
  extern s32 v_comp_temp_s32[2]     = {BME280_INIT_VALUE, BME280_INIT_VALUE};
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:118:13: warning: 'v_comp_press_u32' initialized and declared 'extern'
  extern u32 v_comp_press_u32[2]    = {BME280_INIT_VALUE, BME280_INIT_VALUE};
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:120:13: warning: 'v_comp_humidity_u32' initialized and declared 'extern'
  extern u32 v_comp_humidity_u32[2] = {BME280_INIT_VALUE, BME280_INIT_VALUE};
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:122:13: warning: 'com_rslt' initialized and declared 'extern'
  extern s32 com_rslt = ERROR;
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c: In function 'MainTask':
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:319:34: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
       HAL_UART_Transmit(&huart5, aBuffer,  19, 5000);
                                  ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:24:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:322:34: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
       HAL_UART_Transmit(&huart5, "In BASIC_HelloWorld \n", 21, 5000);
                                  ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:24:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c'
' '
'Building file: ../Application/User/bme280.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Application/User/bme280.d" -MT"Application/User/bme280.o" -o "Application/User/bme280.o" "../Application/User/bme280.c"
'Finished building: ../Application/User/bme280.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Application/User/main.d" -MT"Application/User/main.o" -o "Application/User/main.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c"
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c: In function 'main':
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:234:31: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
    HAL_UART_Transmit(&huart5, aCharBuffer,  23, 5000);
                               ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:339:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, "Set Oversampling Humidity erfolgreich \n", 39, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:344:28: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
     sprintf ( aCharBuffer, "retval of SetOversampHum:%2d \n", com_rslt);
                            ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:344:28: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:346:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, aCharBuffer,  29, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:351:28: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
     sprintf ( aCharBuffer, "retval of SetPower:%2d \n", com_rslt);
                            ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:351:28: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:353:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, aCharBuffer,  23, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:359:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, "Set Pressure Oversampling erfolgreich \n", 39, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:367:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, "Set Temperature Oversampling erfolgreich \n", 42, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:376:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, "*********** Read Versuch fehlgeschlagen \n", 41, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:382:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, aCharBuffer,  12, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:391:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, aCharBuffer,  12, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:407:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:414:28: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
     sprintf ( aCharBuffer, "uTemp:   %6d   \n", uTemp );
                            ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:414:28: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:416:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:424:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:430:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:438:35: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
        HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                   ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:444:37: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
          HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                     ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:449:29: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
  HAL_UART_Transmit(&huart5, "Ende in Loop STEM \n",  19, 5000);
                             ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:452:29: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
  HAL_UART_Transmit(&huart5, "                  \n",  19, 5000);
                             ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:480:14: warning: pointer targets in passing argument 1 of 'sprintf' differ in signedness [-Wpointer-sign]
     sprintf( aTxBuffer, "Vor Error Handler \n");
              ^
In file included from c:\ac6\systemworkbench\plugins\fr.ac6.mcu.externaltools.arm-none.win32_1.7.0.201602121829\tools\compiler\arm-none-eabi\include\stdio.h:29:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_def.h:50,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_rcc.h:47,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:246,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
c:\ac6\systemworkbench\plugins\fr.ac6.mcu.externaltools.arm-none.win32_1.7.0.201602121829\tools\compiler\arm-none-eabi\include\stdio.h:225:5: note: expected 'char * restrict' but argument is of type 'uint8_t * {aka unsigned char *}'
 int _EXFUN(sprintf, (char *__restrict, const char *__restrict, ...)
     ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:494:14: warning: pointer targets in passing argument 1 of 'sprintf' differ in signedness [-Wpointer-sign]
     sprintf( aTxBuffer,"I2C3 Not Ready ");
              ^
In file included from c:\ac6\systemworkbench\plugins\fr.ac6.mcu.externaltools.arm-none.win32_1.7.0.201602121829\tools\compiler\arm-none-eabi\include\stdio.h:29:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_def.h:50,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_rcc.h:47,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:246,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
c:\ac6\systemworkbench\plugins\fr.ac6.mcu.externaltools.arm-none.win32_1.7.0.201602121829\tools\compiler\arm-none-eabi\include\stdio.h:225:5: note: expected 'char * restrict' but argument is of type 'uint8_t * {aka unsigned char *}'
 int _EXFUN(sprintf, (char *__restrict, const char *__restrict, ...)
     ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:495:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, "I2C3 Not Ready \n", 16, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:500:14: warning: pointer targets in passing argument 1 of 'sprintf' differ in signedness [-Wpointer-sign]
     sprintf( aTxBuffer, "MX_I2C3 OK        \n");
              ^
In file included from c:\ac6\systemworkbench\plugins\fr.ac6.mcu.externaltools.arm-none.win32_1.7.0.201602121829\tools\compiler\arm-none-eabi\include\stdio.h:29:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_def.h:50,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_rcc.h:47,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:246,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
c:\ac6\systemworkbench\plugins\fr.ac6.mcu.externaltools.arm-none.win32_1.7.0.201602121829\tools\compiler\arm-none-eabi\include\stdio.h:225:5: note: expected 'char * restrict' but argument is of type 'uint8_t * {aka unsigned char *}'
 int _EXFUN(sprintf, (char *__restrict, const char *__restrict, ...)
     ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:511:34: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
       HAL_UART_Transmit(&huart5, "*********** Read Versuch fehlgeschlagen \n", 41, 5000);
                                  ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:523:30: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
   HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                              ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:530:35: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
        HAL_UART_Transmit(&huart5, "*********** Read Versuch gelungen \n", 35, 5000);
                                   ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:536:36: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
         HAL_UART_Transmit(&huart5, aCharBuffer,  12, 5000);
                                    ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:545:37: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
          HAL_UART_Transmit(&huart5, aCharBuffer,  12, 5000);
                                     ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:561:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:568:29: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
      sprintf ( aCharBuffer, "uTemp:   %6d   \n", uTemp );
                             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:568:29: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:570:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:581:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:587:34: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
       HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                  ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:595:36: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
         HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                    ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:601:38: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
           HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                      ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:606:30: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
   HAL_UART_Transmit(&huart5, "Ende in Loop      \n",  19, 5000);
                              ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:609:30: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
   HAL_UART_Transmit(&huart5, "                  \n",  19, 5000);
                              ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c: In function 'MX_I2C3_Init':
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:900:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, "MX_I2C3 AZ \n", 12, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c: At top level:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:95:12: warning: 'v_stand_by_time_u8' defined but not used [-Wunused-variable]
  static u8 v_stand_by_time_u8      = BME280_INIT_VALUE;
            ^
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/stm32f4xx_it.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Application/User/stm32f4xx_it.d" -MT"Application/User/stm32f4xx_it.o" -o "Application/User/stm32f4xx_it.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/stm32f4xx_it.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/stm32f4xx_it.c'
' '
'Building target: STM32F429I_DISCO_MB1075.elf'
'Invoking: MCU GCC Linker'
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -L"D:\HAL\STM32Cube_FW_F4_V1.14.0\Middlewares\ST\STemWin\Lib"  -specs=nosys.specs -specs=nano.specs -T"../STM32F429ZITx_FLASH.ld" -Wl,-Map=output.map -Wl,--gc-sections -lm -o "STM32F429I_DISCO_MB1075.elf" @"objects.list"  -l:STemWin532_CM4_GCC.a
Application/User/main.o: In function `main':
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:285: undefined reference to `HAL_RTC_Init'
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:299: undefined reference to `HAL_RTC_SetTime'
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:309: undefined reference to `HAL_RTC_SetDate'
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:326: undefined reference to `HAL_RTC_SetAlarm'
collect2.exe: error: ld returned 1 exit status
make: *** [STM32F429I_DISCO_MB1075.elf] Error 1

10:24:52 Build Finished (took 31s.613ms)
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_io.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_io.d" -MT"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_io.o" -o "Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_io.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_io.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_io.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_lcd.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_lcd.d" -MT"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_lcd.o" -o "Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_lcd.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_lcd.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_lcd.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_sdram.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_sdram.d" -MT"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_sdram.o" -o "Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_sdram.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_sdram.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_sdram.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_ts.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_ts.d" -MT"Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_ts.o" -o "Drivers/BSP/STM324x9I_DISCO/stm32f429i_discovery_ts.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_ts.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery_ts.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/Components/ili9341/ili9341.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Drivers/BSP/Components/ili9341.d" -MT"Drivers/BSP/Components/ili9341.o" -o "Drivers/BSP/Components/ili9341.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/Components/ili9341/ili9341.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/Components/ili9341/ili9341.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/Components/stmpe811/stmpe811.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Drivers/BSP/Components/stmpe811.d" -MT"Drivers/BSP/Components/stmpe811.o" -o "Drivers/BSP/Components/stmpe811.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/Components/stmpe811/stmpe811.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/Components/stmpe811/stmpe811.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Application/User/BASIC_HelloWorld.d" -MT"Application/User/BASIC_HelloWorld.o" -o "Application/User/BASIC_HelloWorld.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c"
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:108:12: warning: 'v_stand_by_time_u8' initialized and declared 'extern'
  extern u8 v_stand_by_time_u8      = BME280_INIT_VALUE;
            ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:110:13: warning: 'v_data_uncomp_temp_s32' initialized and declared 'extern'
  extern s32 v_data_uncomp_temp_s32 = BME280_INIT_VALUE;
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:112:13: warning: 'v_data_uncomp_pres_s32' initialized and declared 'extern'
  extern s32 v_data_uncomp_pres_s32 = BME280_INIT_VALUE;
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:114:13: warning: 'v_data_uncomp_hum_s32' initialized and declared 'extern'
  extern s32 v_data_uncomp_hum_s32  = BME280_INIT_VALUE;
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:116:13: warning: 'v_comp_temp_s32' initialized and declared 'extern'
  extern s32 v_comp_temp_s32[2]     = {BME280_INIT_VALUE, BME280_INIT_VALUE};
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:118:13: warning: 'v_comp_press_u32' initialized and declared 'extern'
  extern u32 v_comp_press_u32[2]    = {BME280_INIT_VALUE, BME280_INIT_VALUE};
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:120:13: warning: 'v_comp_humidity_u32' initialized and declared 'extern'
  extern u32 v_comp_humidity_u32[2] = {BME280_INIT_VALUE, BME280_INIT_VALUE};
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:122:13: warning: 'com_rslt' initialized and declared 'extern'
  extern s32 com_rslt = ERROR;
             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c: In function 'MainTask':
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:319:34: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
       HAL_UART_Transmit(&huart5, aBuffer,  19, 5000);
                                  ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:24:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:322:34: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
       HAL_UART_Transmit(&huart5, "In BASIC_HelloWorld \n", 21, 5000);
                                  ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery/stm32f429i_discovery.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c:24:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/BASIC_HelloWorld.c'
' '
'Building file: ../Application/User/bme280.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Application/User/bme280.d" -MT"Application/User/bme280.o" -o "Application/User/bme280.o" "../Application/User/bme280.c"
'Finished building: ../Application/User/bme280.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Application/User/main.d" -MT"Application/User/main.o" -o "Application/User/main.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c"
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c: In function 'main':
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:234:31: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
    HAL_UART_Transmit(&huart5, aCharBuffer,  23, 5000);
                               ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:339:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, "Set Oversampling Humidity erfolgreich \n", 39, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:344:28: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
     sprintf ( aCharBuffer, "retval of SetOversampHum:%2d \n", com_rslt);
                            ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:344:28: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:346:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, aCharBuffer,  29, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:351:28: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
     sprintf ( aCharBuffer, "retval of SetPower:%2d \n", com_rslt);
                            ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:351:28: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:353:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, aCharBuffer,  23, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:359:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, "Set Pressure Oversampling erfolgreich \n", 39, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:367:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, "Set Temperature Oversampling erfolgreich \n", 42, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:376:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, "*********** Read Versuch fehlgeschlagen \n", 41, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:382:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, aCharBuffer,  12, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:391:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, aCharBuffer,  12, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:407:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:414:28: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
     sprintf ( aCharBuffer, "uTemp:   %6d   \n", uTemp );
                            ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:414:28: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:416:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:424:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:430:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:438:35: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
        HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                   ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:444:37: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
          HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                     ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:449:29: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
  HAL_UART_Transmit(&huart5, "Ende in Loop STEM \n",  19, 5000);
                             ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:452:29: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
  HAL_UART_Transmit(&huart5, "                  \n",  19, 5000);
                             ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:480:14: warning: pointer targets in passing argument 1 of 'sprintf' differ in signedness [-Wpointer-sign]
     sprintf( aTxBuffer, "Vor Error Handler \n");
              ^
In file included from c:\ac6\systemworkbench\plugins\fr.ac6.mcu.externaltools.arm-none.win32_1.7.0.201602121829\tools\compiler\arm-none-eabi\include\stdio.h:29:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_def.h:50,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_rcc.h:47,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:246,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
c:\ac6\systemworkbench\plugins\fr.ac6.mcu.externaltools.arm-none.win32_1.7.0.201602121829\tools\compiler\arm-none-eabi\include\stdio.h:225:5: note: expected 'char * restrict' but argument is of type 'uint8_t * {aka unsigned char *}'
 int _EXFUN(sprintf, (char *__restrict, const char *__restrict, ...)
     ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:494:14: warning: pointer targets in passing argument 1 of 'sprintf' differ in signedness [-Wpointer-sign]
     sprintf( aTxBuffer,"I2C3 Not Ready ");
              ^
In file included from c:\ac6\systemworkbench\plugins\fr.ac6.mcu.externaltools.arm-none.win32_1.7.0.201602121829\tools\compiler\arm-none-eabi\include\stdio.h:29:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_def.h:50,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_rcc.h:47,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:246,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
c:\ac6\systemworkbench\plugins\fr.ac6.mcu.externaltools.arm-none.win32_1.7.0.201602121829\tools\compiler\arm-none-eabi\include\stdio.h:225:5: note: expected 'char * restrict' but argument is of type 'uint8_t * {aka unsigned char *}'
 int _EXFUN(sprintf, (char *__restrict, const char *__restrict, ...)
     ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:495:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, "I2C3 Not Ready \n", 16, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:500:14: warning: pointer targets in passing argument 1 of 'sprintf' differ in signedness [-Wpointer-sign]
     sprintf( aTxBuffer, "MX_I2C3 OK        \n");
              ^
In file included from c:\ac6\systemworkbench\plugins\fr.ac6.mcu.externaltools.arm-none.win32_1.7.0.201602121829\tools\compiler\arm-none-eabi\include\stdio.h:29:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_def.h:50,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_rcc.h:47,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:246,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
c:\ac6\systemworkbench\plugins\fr.ac6.mcu.externaltools.arm-none.win32_1.7.0.201602121829\tools\compiler\arm-none-eabi\include\stdio.h:225:5: note: expected 'char * restrict' but argument is of type 'uint8_t * {aka unsigned char *}'
 int _EXFUN(sprintf, (char *__restrict, const char *__restrict, ...)
     ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:511:34: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
       HAL_UART_Transmit(&huart5, "*********** Read Versuch fehlgeschlagen \n", 41, 5000);
                                  ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:523:30: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
   HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                              ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:530:35: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
        HAL_UART_Transmit(&huart5, "*********** Read Versuch gelungen \n", 35, 5000);
                                   ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:536:36: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
         HAL_UART_Transmit(&huart5, aCharBuffer,  12, 5000);
                                    ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:545:37: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
          HAL_UART_Transmit(&huart5, aCharBuffer,  12, 5000);
                                     ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:561:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:568:29: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
      sprintf ( aCharBuffer, "uTemp:   %6d   \n", uTemp );
                             ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:568:29: warning: format '%d' expects argument of type 'int', but argument 3 has type 's32 {aka long int}' [-Wformat=]
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:570:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:581:33: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
      HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                 ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:587:34: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
       HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                  ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:595:36: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
         HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                    ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:601:38: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
           HAL_UART_Transmit(&huart5, aCharBuffer,  19, 5000);
                                      ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:606:30: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
   HAL_UART_Transmit(&huart5, "Ende in Loop      \n",  19, 5000);
                              ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:609:30: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
   HAL_UART_Transmit(&huart5, "                  \n",  19, 5000);
                              ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c: In function 'MX_I2C3_Init':
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:900:32: warning: pointer targets in passing argument 2 of 'HAL_UART_Transmit' differ in signedness [-Wpointer-sign]
     HAL_UART_Transmit(&huart5, "MX_I2C3 AZ \n", 12, 5000);
                                ^
In file included from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/stm32f4xx_hal_conf.h:366:0,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal.h:48,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc/main.h:52,
                 from D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:48:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_uart.h:647:19: note: expected 'uint8_t * {aka unsigned char *}' but argument is of type 'char *'
 HAL_StatusTypeDef HAL_UART_Transmit(UART_HandleTypeDef *huart, uint8_t *pData, uint16_t Size, uint32_t Timeout);
                   ^
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c: At top level:
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:95:12: warning: 'v_stand_by_time_u8' defined but not used [-Wunused-variable]
  static u8 v_stand_by_time_u8      = BME280_INIT_VALUE;
            ^
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c'
' '
'Building file: D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/stm32f4xx_it.c'
'Invoking: MCU GCC Compiler'
D:\HAL\STM32Cube_FW_F4_V1.14.0\Projects\STM32F429I-Discovery\Applications\STemWin\STemWin_HelloWorld\SW4STM32\STM32F429I_DISCO_MB1075\Debug
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -DSTM32F429xx -DUSE_STM32F429I_DISCO -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Src" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Device/ST/STM32F4xx/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/CMSIS/Include" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/STM32F4xx_HAL_Driver/Inc" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Drivers/BSP/STM32F429I-Discovery" -I"D:/HAL/STM32Cube_FW_F4_V1.14.0/Middlewares/ST/STemWin/inc" -I"D:/AZI/Wetterstation/BME280_Source"  -Os -g3 -Wall -fmessage-length=0 -ffunction-sections -c -fmessage-length=0 -MMD -MP -MF"Application/User/stm32f4xx_it.d" -MT"Application/User/stm32f4xx_it.o" -o "Application/User/stm32f4xx_it.o" "D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/stm32f4xx_it.c"
'Finished building: D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/stm32f4xx_it.c'
' '
'Building target: STM32F429I_DISCO_MB1075.elf'
'Invoking: MCU GCC Linker'
arm-none-eabi-gcc -mcpu=cortex-m4 -mthumb -mfloat-abi=hard -mfpu=fpv4-sp-d16 -L"D:\HAL\STM32Cube_FW_F4_V1.14.0\Middlewares\ST\STemWin\Lib"  -specs=nosys.specs -specs=nano.specs -T"../STM32F429ZITx_FLASH.ld" -Wl,-Map=output.map -Wl,--gc-sections -lm -o "STM32F429I_DISCO_MB1075.elf" @"objects.list"  -l:STemWin532_CM4_GCC.a
Application/User/main.o: In function `main':
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:285: undefined reference to `HAL_RTC_Init'
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:299: undefined reference to `HAL_RTC_SetTime'
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:309: undefined reference to `HAL_RTC_SetDate'
D:/HAL/STM32Cube_FW_F4_V1.14.0/Projects/STM32F429I-Discovery/Applications/STemWin/STemWin_HelloWorld/Src/main.c:326: undefined reference to `HAL_RTC_SetAlarm'
collect2.exe: error: ld returned 1 exit status
make: *** [STM32F429I_DISCO_MB1075.elf] Error 1

10:24:52 Build Finished (took 31s.613ms)